VAIO User Guide

Task

# Replacing the AA Battery of the Keyboard

Change the AA battery in the keyboard when the battery power becomes low.

1. Set the power switch of the keyboard to OFF.

1. Turn over the keyboard, and then push the center of the cover in the direction shown in the illustration below.

1. Remove the old battery and insert a new AA alkaline battery (minus (-) end first), then close the cover.

1. Set the power switch of the keyboard to ON.

Note

- Use a new AA alkaline replacement battery.

- If you do not intend to use the keyboard for a while, set the power switch of the keyboard to OFF. If you do not intend to use the keyboard for an extended period of time, remove its AA battery.

- When the battery power becomes low, replace with a new AA battery promptly. Keeping a depleted battery in the keyboard may cause battery leakage.

- Since the keyboard cannot be used with a commercially available rechargeable battery, use a non-rechargeable AA battery. If you use a rechargeable battery, battery leakage may occur, resulting in a malfunction.

- Do not recharge a dry cell AA battery.

- Refer to the supplied safety information manual.

Related Topic
Parts and Controls of the Keyboard
Checking the Remaining Battery Power of the Keyboard