# Personal Computer VAIO Fit 13A/14A/15ASVF13N1/SVF14N1/SVF15N1

## Replacing the Battery of the Pen (Digitizer Stylus supplied models)

Replace the battery when the pen (Digitizer Stylus) begins to function incorrectly.

Based on usage of approximately 4 hours a day, expect to replace the battery every 18 months. Use an LR61 (LR8D425) alkaline battery.

1. Remove the Tail cap from the pen, then remove the battery.

2. Insert the battery into the pen with the + side toward the nib.

3. Reattach the Tail cap.

#### Note

- Do not remove the Tail cap except for when replacing the battery.

- If you do not intend to use the pen for a while, remove the battery.

- The pen should not be used with a commercially available rechargeable battery. Using a rechargeable battery may result in battery leakage and malfunction.

- When the battery power becomes low, replace with a new battery promptly. Keeping a depleted battery in the pen may cause battery leakage.

- Do not attempt to recharge a battery.

- Refer to the supplied safety manual.

Go to Page Top

### Related Topic

- How to Use the Pen (Digitizer Stylus supplied models)

Go to Page Top