#

# i-Manual online

- Print
- Font Size

- Top Page >
- Parts Description >
- Back

# Back

- LAN
- / PC IN
- HDMI IN 1/4
- DIGITAL AUDIO OUT (OPTICAL)
- (VAR/FIX)
- / COMPONENT IN
- / AV 1/2
- 3D SYNC

1. LAN

   Connects to an existing network using an Ethernet cable.

2. / PC IN

   Connect with a PC cable with ferrites, and an audio cable.

   ####

   - It is recommended to use a PC cable with ferrites, such as the “Connector, D-sub 15” (ref. 1-793-504-11, available in Sony Service Centre), or an equivalent.
3. HDMI IN 1/4

   HDMI (High-Definition Multimedia Interface) provides an uncompressed, all-digital audio/video interface between this TV and any HDMI-equipped audio/video equipment. In addition, when you connect the equipment that is compatible with “Control for HDMI”, communication with the connected equipment is supported.

   ####

   - Be sure to use only an authorised HDMI cable bearing the HDMI logo.
   - If connecting a digital audio system that is compatible with Audio Return Channel (ARC) technology, use the HDMI IN 1. If not, an additional connection with DIGITAL AUDIO OUT (OPTICAL) is necessary.
   - If the equipment has a DVI jack (socket), connect it to the HDMI IN 4 through a DVI - HDMI adaptor interface (not supplied), and connect the equipment’s audio out jacks (sockets) to the PC/HDMI 4 AUDIO IN which is located in the PC IN.
4. DIGITAL AUDIO OUT (OPTICAL)

   You can listen to TV sound on the connected Home theatre system with digital input.

5. (VAR/FIX)

   Connect with an audio cable. You can listen to TV sound on the connected Hi-Fi audio equipment.

6. / COMPONENT IN

   Connect with a component video cable for video signals. Audio connection is also required for audio signals.

7. / AV 1/2

   Connect with a SCART cable. When you connect an analogue decoder, the TV tuner outputs scrambled signals to the decoder, and the decoder unscrambles the signals before outputting them.

8. 3D SYNC

   Connect to the 3D Sync Transmitter that is sold separately.

9. RF input that connects to your cable or antenna (aerial).

   ####

   - For satellite-compatible models, a satellite input is also available.

Copyright 2010 Sony Corporation