#

# i-Manual online

- Print
- Font Size

- Top Page >
- Parts Description >
- Front

# Front

- Light sensor
- Remote control sensor
- (Picture off/Timer)
- (Standby)
- I (Power)
- 3D Sync Transmitter

1. Light sensor

   Senses room light level and adjusts the screen brightness accordingly.

   Do not put anything near the sensor. Doing so may affect its function.

2. Remote control sensor

   Receives signals from the remote.

   Do not put anything near the sensor. Doing so may affect its function.

3. (Picture off/Timer)

   Lights up in green when you select [Picture Off].

   Lights up in orange when you set the timer.

   Lights up in and/or blinks orange during a software upgrade.

   Lights up in orange when you set the timer recording on the USB HDD device or equipment connected via SCART connection.

   ####

   - The USB HDD recording function may not be available depending on your model/region/country.
4. (Standby)

   Lights up in red when your TV is in standby mode, PC power saving mode or during a software upgrade.

5. I (Power)

   Lights up in green when the TV is on.

   Lights up in red when timer recording to the USB HDD device or equipment connected via SCART connection is in progress.

   ####

   - The USB HDD recording function may not be available depending on your model/region/country.
6. 3D Sync Transmitter

   Emits the 3D sync signal.

   ####

   - Do not put anything in front of the 3D Sync Transmitter. Doing so may affect its function.

Copyright 2011 Sony Corporation