Cyber-shot User Guide
Print
Top page > Shooting > Using shooting functions > Cont. Shooting/Self-Timer

## Cont. Shooting/Self-Timer

Automatic shooting with Self-portrait timer
You can select Single (single-image), Continuous Shooting or Bracket as the shooting mode.

1. Press / (Cont. Shooting/Self-Timer) on the control wheel.

1. Select the desired mode with the control wheel.

| (Single Shooting) | The camera shoots a single image without using the self-timer.
| (Continuous Shooting) | The camera shoots up to 10 continuous frames in one burst when you hold down the shutter button.
| (Bracket) | The camera shoots a series of 3 images each with a different setting.
| (10sec) | Sets the self-timer to a 10-second delay. When you press the shutter button, the self-timer lamp flashes and a beep sounds until the shutter operates. To cancel, press again.
| (2sec) | Sets the self-timer to a 2-second delay.
| (Self-portrait One Person) | Sets the self-timer to Self-portrait timer. When the camera detects the specified number of faces, a beep sounds, and the shutter operates 2 seconds later.
| (Self-portrait Two People)
| (Self-Timer: Continuous Shooting) | The camera shoots 10 continuous frames 10 seconds later after you press the shutter button.
| (Self-Timer (Bracket)) | The camera starts bracket shooting 10 seconds later after you press the shutter button.

Tips for preventing blur
If your hands or body moves while holding the camera and pressing the shutter button, “Camera shake” occurs.
Camera shake occurs frequently under low-light or slow shutter speed conditions, such as those encountered in (Night Portrait) or (Night Scene) mode.
To reduce camera shake, set the self-timer to a 2-second delay and brace your arms against your sides after pressing the shutter button.
Notes

- [Flash] is set to [Off] in continuous or bracket shooting mode.

- When [Continuous Shooting] is selected, [Focus], [White Balance], and [EV] are adjusted for the first image, and these settings are also used for the other images.

- When the battery level is low, or when the internal memory or a memory card is full, the burst stops.

- [VGA] image size will be set while recording on internal memory.

### Automatic shooting with Self-portrait timer

Point the lens at yourself so that the selected number of faces are reflected in the screen. The shutter operates automatically. Do not move your camera after the beep sounds.

- You can also shoot an image by pressing the shutter button during this operation.

Related Topic
Functions not available in some REC modes
Cont. Shooting Interval
Bracket Setting
Back to top