Cyber-shot User Guide
Print
Top page > Shooting > Shooting still images > Zoom (Still images)

## Zoom (Still images)

Available zoom
Zoom scale
Enlarges images with the W/T (zoom) lever when shooting. The camera’s optical zoom function can enlarge images up to 30×.
Optical zoom allows you to enlarge an image without deteriorating its original quality.
You can set the zoom using the W/T (zoom) lever or the manual ring.
Zooming using the W/T (zoom) lever

1. Set the camera to shooting mode.

1. Slide the W/T (zoom) lever.

Slide the lever to the T side to zoom in, or to the W side to zoom out.
Zooming using the manual ring

1. Set the Zoom/Focus switch to AF/ZOOM.

1. Turn the manual ring.

Turn the manual ring to T side to zoom in, W side to zoom out.
Note

- Zoom is locked to the W side for shooting in the following situations:

- In [iSweep Panorama]

- In [3D Sweep Panorama]

- In [Sweep Multi Angle]

### Available zoom

You can combine certain zoom settings to zoom in at high magnification. The icon on the screen changes in accordance with the zoom you use.

1. Zoom with the original image quality

(You can shoot still images without deteriorating the original image quality even if the optical zoom scale exceeds 30× magnification.)

1. () [Clear Image Zoom]:

Zoom with close to the original image quality [Details]

1. () [Digital Zoom]:

Less than the original image quality [Details]

| Operation | Settings | Zoom bar
A | Using optical zoom only | Still Image Size: [18M] [Clear Image Zoom]: [Off] [Digital Zoom]: [Off] |
B | Zooming images without deterioration | Still Image Size: other than [18M] [Clear Image Zoom]: [Off] [Digital Zoom]: [Off] |
C | Shooting clear images using [Clear Image Zoom] (close to the original image quality) | [Clear Image Zoom]: [On] [Digital Zoom]: [Off] |
D | Zooming to the maximum zoom range | [Clear Image Zoom]: [On] [Digital Zoom]: [On] [Clear Image Zoom] may not be available for some settings. [Details] | When [Clear Image Zoom] is not available

### Zoom scale

The supported zoom scales are different depending on the settings or the image size. The table below summarizes the zoom scales when [Clear Image Zoom] and [Digital Zoom] are set to [On].

Image size | Operation | D: Zoom with maximum zoom scale*1
A: Optical zoom | B: Zoom by range without deterioration (including 30× optical zoom) | C: Zoom with [Clear Image Zoom] [On]
18M | 30× | 30× | 60× | 120×
10M | 30× | 40× | 80× | 161×
5M | 30× | 56× | 113× | 226×
VGA | 30× | 229× | 459× | 459×*2
16:9(13M) | 30× | 30× | 60× | 120×
16:9(2M) | 30× | 76× | 153× | 306×

*1 The maximum zoom scale is the total zoom magnification that can be achieved when zoom scale without deterioration (including 30× optical zoom), [Clear Image Zoom] and [Digital Zoom] are used in combination. The maximum zoom scale varies depending on the settings. The maximum zoom scale for the default setting is the same as when [Clear Image Zoom] is [On]. [Details]
*2 When [Still Image Size] is set to [VGA], [Digital Zoom] is limited; the maximum zoom scale is 459×.
Notes

- The default setting for [Clear Image Zoom] is [On].

- The default setting for [Digital Zoom] is [Off]. Set [Digital Zoom] to [On] to enlarge images even with deterioration. [Details]

- The default setting for [Still Image Size] is [18M]. To change the zoom scale, change [Still Image Size]. [Details]

- Zoom functions other than the optical zoom are not available when shooting in the following situations:

- In [iSweep Panorama]

- In [Picture Effect]

- In [Background Defocus]

- When the Smile Shutter function is activated.

- When [Self-Timer] is set to [Self-portrait One Person] or [Self-portrait Two People].

- When (Backlight Correction HDR) or (Advanced Sports Shooting) mode is selected in Scene Selection.

- The Face Detection function does not operate when you use other than the optical zoom.

Back to top