Cyber-shot User Guide
Print
Top page > Using with your computer > Recommended computer environment > Recommended computer environment

## Recommended computer environment

The following computer environment is recommended when using the software “PlayMemories Home” (Windows) and “Music Transfer” (Windows/Mac) and when importing images via a USB connection.

#### Windows

OS (pre-installed) | Microsoft Windows XP*1 SP3/Windows Vista*2 SP2/Windows 7 SP1
CPU | Intel Pentium III 800 MHz or faster (For playing/editing the High Definition movies: Intel Core Duo 1.66 GHz or faster/Intel Core 2 Duo 1.66 GHz or faster (Intel Core 2 Duo 2.26 GHz or faster is required when processing AVC HD (FX/FH) movies and Intel Core 2 Duo 2.40 GHz or faster is required when processing AVC HD (PS) movies.))
Memory | Windows XP: 512 MB or more (1 GB or more is recommended.) Windows Vista/Windows 7: 1 GB or more
Hard Disk (Disk space required for installation) | Approximately 500 MB
Display | 1,024×768 dots or more

*1 64-bit editions and Starter (Edition) are not supported.
Windows Image Mastering API (IMAPI) Ver.2.0 or later is required to create a disc by installing the “Expanded Feature.”
*2 Starter (Edition) is not supported.

#### Mac

OS (pre-installed) | USB Connection: Mac OS X v10.3 to v10.7 Music Transfer: Mac OS X v10.4 to v10.7*

* Equipped with Intel processor
Notes

- Operation is not assured in an environment based on an upgrade of the operating systems described above or in a multi-boot environment.

- If you connect two or more USB devices to a single computer at the same time, some devices, including the camera, may not operate, depending on the types of USB devices you are using.

- Connecting the camera using a USB interface that is compatible with Hi-Speed USB (USB 2.0) allows advanced transfer (high speed transfer), as the camera is compatible with Hi-Speed USB (USB 2.0).

- When your computer resumes activity from suspend or sleep mode, communication between the camera and your computer may not recover at the same time.

Back to top