Cyber-shot User Guide
Print
Top page > Using MENU items (Shooting) > MENU items (Shooting) > Easy Mode

## Easy Mode

On Scene Recognition
Shooting functions available in Easy Mode (Shooting)
Allows you to shoot still images using the minimum necessary functions.
The text size increases and indicators become easier to see.

1. Set the mode dial to (Intelligent Auto).

1. MENU (Easy Mode) on the control wheel

1. [OK]

1. Shoot with the shutter button.

To end Easy Mode, MENU [Exit Easy Mode]
On Easy Mode (Viewing)
When you press the (Playback) button in Easy Mode, the playback screen text becomes larger and easier to see.
Delete currently displayed image:
/ (Delete) button [OK] on the control wheel
Select between [1 image] and [All]:
MENU [Delete] on the control wheel desired mode
You can delete currently displayed image with [1 image] and delete all images in the selected date range or internal memory (if selected) with [All].
Use GPS function (DSC-HX20V/HX30V only):
You can select the setting for [GPS setting] on the MENU screen in Easy Mode.
For details on the function, see [GPS setting]. [Details]
MENU [GPS setting] desired mode
Select between [On] and [Off] mode.

- [View Mode] is set to [Date View] when using a memory card.

- When boarding an airplane while the camera is set to Easy Mode, set [GPS setting] to [Off].

Note

- The battery power may decrease faster because the screen brightness increases automatically.

### On Scene Recognition

Scene Recognition operates in Easy Mode. This function lets the camera automatically recognize the shooting conditions and shoot the image.

### Shooting functions available in Easy Mode (Shooting)

MOVIE (Movie) button | Allows you to record movies with their audio.
Still Image Size | MENU [Still Image Size] on the control wheel desired mode Select between [Large] or [Small] size.
GPS setting (DSC-HX20V/HX30V only) | MENU [GPS setting] on the control wheel desired mode Select between [On] or [Off] mode.
Self-Timer | on the control wheel desired mode Select between [On] or [Off] mode.
Flash | on the control wheel desired mode Select between [Auto] or [Off] mode.

Related Topic
Scene Recognition
GPS setting (DSC-HX20V/HX30V only)
Back to top