Cyber-shot User Guide
Print
Top page > Shooting > Functions that can be selected using the Fn button > Flash Comp.

## Flash Comp.

Adjusts the amount of flash light. Separately to the exposure compensation, flash compensation changes the amount of flash light to change the exposure for the main subject within the range of flash light.

1. Fn (Flash Comp.) desired value

Adjusting the value to the + side increases the flash level and to the – side decreases the flash level.
What is the difference between exposure compensation and flash compensation?
Exposure compensation changes the amount of flash light along with the change of the shutter speed, aperture, and ISO (when [ISO] is set to [ISO AUTO]). Flash compensation changes the amount of flash light only.
Related Topic
Still shooting menu items not available in some REC modes
Back to top