Cyber-shot User Guide
Print
Top page > Using MENU items (Shooting) > Still shooting menu > Long Exposure NR

## Long Exposure NR

When you set the shutter speed to 1 second or longer (Long exposure shooting), noise reduction is turned on for the same duration that the shutter is open. This is to reduce the grainy noise typical in a long exposure.

1. MENU 2 [Long Exposure NR] desired mode

| On | Activates noise reduction for the same duration that the shutter is open. When noise reduction is in progress, a message appears and you cannot take another picture. Select this to prioritize the image quality.
| Off | Does not use [Long Exposure NR]. Select this to prioritize the timing of shooting.

Notes

- Even when [Long Exposure NR] is set to [On], noise reduction is not available in the following situations:

- In [Cont. Shooting]

- In [Spd Priority Cont.]

- In [Bracket: Cont.]

- When [Scene Selection] is set to (Sports Action) or (Hand-held Twilight)

- In [Sweep Panorama] mode

Related Topic
Still shooting menu items not available in some REC modes
Back to top