Cyber-shot User Guide
Print
Top page > Shooting > Setting REC mode > Functions not available in some REC modes

## Functions not available in some REC modes

Functions available in REC modes
Functions available in [Scene Selection]
In the table below, a check mark indicates a function that can be changed, while — indicates function that cannot be changed. The icons below [Flash Mode] and [Drive Mode] indicate the available modes.
When the shooting modes below are registered and recalled by setting the mode dial to 1/2/3, the conditions for whether settings can be changed or not remain the same as in the table below.

### Functions available in REC modes

| Flash Mode | Smile/Face Detect. | Tracking focus | Drive Mode | Exposure Comp.
(Intelligent Auto)/ (Superior Auto) |  |  |  |  | —
(Program Auto) | *1 |  |  |  |
(Aperture Priority) | *1 |  |  |  |
(Shutter Priority) | *1 |  |  |  |
(Manual Exposure) | *1 |  |  |  | —
(Movie) |  | *2 |  |  | *3
(Sweep Panorama) |  | — | — |  |

*1 Wireless flash shooting is not available with the built-in flash.
*2 Smile Shutter cannot be selected.
*3 Exposure value can be set from –2.0EV to +2.0EV.

### Functions available in [Scene Selection]

| Flash Mode | Smile/Face Detect. | Tracking focus | Drive Mode | Exposure Comp.
(Portrait) |  |  |  |  | —
(Sports Action) |  |  |  |  | —
(Landscape) |  |  |  |  | —
(Sunset) |  |  |  |  | —
(Night Scene) |  |  |  |  | —
(Hand-held Twilight) |  | * | — |  | —
(Night Portrait) |  |  |  |  | —

* Smile Shutter cannot be selected.
Back to top