Cyber-shot User Guide
Print
Top page > Using MENU items (Shooting) > MENU items (Shooting) > EV

## EV

You can adjust the exposure manually in 1/3 EV steps in a range of –2.0 EV to +2.0 EV.

1. MENU (EV)

Depending on the REC mode, this is set using buttons displayed on the left side of the screen.

1. Touch / to adjust exposure [OK].

You can also adjust the exposure by touching of the adjustment bar and dragging to the right or left.
Adjusting the exposure for better looking images
A: Overexposure (too much light)
B: Correct exposure
C: Underexposure (too little light)

- When the image shot is overexposed, adjust [EV] to the minus side.

- When the image shot is underexposed, adjust [EV] to the plus side.

Notes

- If you shoot a subject in extremely bright or dark conditions, or when you use the flash, the exposure adjustment may not be effective.

- You may not be able to set some MENU items depending on the selected REC mode. For details, see “MENU items not available in some REC modes.” [Details]

Back to top