Cyber-shot User Guide
Print
Top page > Precautions / About this camera > Number of still images and recordable time of movies > Recordable time of movies

## Recordable time of movies

The table below shows the approximate maximum recording times. These are the total times for all movie files.
(h (hour), m (minute))

Quality / Size | Internal memory | Memory card formatted with this camera
Approx. 56 MB | 2 GB | 4 GB | 8 GB | 16 GB | 32 GB
1280x720(Fine) | - | 25 m (20 m) | 50 m (45 m) | 1 h 45 m (1 h 35 m) | 3 h 40 m (3 h 10 m) | 7 h 20 m (6 h 20 m)
1280x720(Standard) | - | 35 m (30 m) | 1 h 10 m (1 h 5 m) | 2 h 20 m (2 h 20 m) | 4 h 40 m (4 h 40 m) | 9 h 25 m (9 h 20 m)
VGA | 2 m (2 m) | 1 h 5 m (1 h 5 m) | 2 h 15 m (2 h 10 m) | 4 h 40 m (4 h 25 m) | 9 h 20 m (8 h 50 m) | 18 h 45 m (17 h 45 m)

The number in ( ) is the minimum recordable time.
Continuous shooting is possible for approximately 29 minutes at one time. The maximum size of a movie file is up to approximately 2 GB.
Notes

- The recordable time of movies varies because the camera is equipped with VBR (Variable Bit Rate), which automatically adjusts image quality depending on the shooting scene. When you record a fast-moving subject, the image is clearer but the recordable time is shorter because more memory is required for recording. The recordable time also varies depending on the shooting conditions, the subject or the image size settings.

- You cannot record movies to the internal memory when the movie image size is [1280x720(Fine)] or [1280x720(Standard)].

Back to top