Cyber-shot User Guide
Print
Top page > Using MENU items (Shooting) > MENU items (Shooting) > Bracket Setting

## Bracket Setting

You can set the type of shooting when [Burst Settings] is set to [Bracket]. In the bracket shooting mode, you can record a series of 3 images with the setting changed. You can select the most suitable image afterwards.

1. MENU (Bracket Setting) desired mode

| (EXP±0.3) | Records a series of 3 images with the exposure shifted in the following order: bright, standard, and dark. The larger the bracket step value, the larger the shift of the exposure value.
| (EXP±0.7)
| (EXP±1.0)
| (White Balance) | Records a series of 3 images with the white balance shifted in the following order: current color tone, toward blue, and toward red. When you set [White Balance] to other than [Auto], the color tone is shifted based on the selected white balance.

Notes

- You cannot select [White Balance] when the mode dial is set to (Scene Selection).

- You may not be able to set some functions or MENU items depending on the selected REC mode. For details, see “Functions not available in some REC modes” [Details] and “MENU items not available in some REC modes.” [Details]

Back to top