Cyber-shot User Guide
Print
Top page > Using MENU items (Shooting) > MENU items (Shooting) > Scene Recognition

## Scene Recognition

Advanced mode
The camera automatically detects shooting conditions, and then takes the shot. When a motion is detected, the ISO sensitivity is increased according to the movement to reduce subject blur. When the camera is set to Intelligent Auto mode, you can select [Advanced] mode, in which the camera automatically shoots two images.
In Scene Recognition, the position of an icon displayed on the screen is different depending on the circumstances. It depends on whether the camera recognizes a scene or condition. If the camera recognizes a scene, icons and guides such as (Portrait), (Infant), (Night Portrait), (Night Scene), (Backlight Portrait), (Backlight), (Landscape), (Macro), (Spotlight) or (Low Light) are displayed on the first line. If the camera recognizes a condition, icons such as (Tripod) or (Move) are displayed on the second line. The camera may recognize both the scene and condition, or just one.

1. MENU (Scene Recognition) desired mode

| (Auto) | When the camera recognizes the scene, it switches to the optimal settings and shoots the image.
| (Advanced) | When the camera recognizes the scene, it switches to the optimal settings. When the camera recognizes (Night Scene), (Night Portrait), (Backlight) or (Backlight Portrait), it automatically changes the setting and shoots another image. When you shoot two images consecutively, the + mark on the icon will turn green. When two frames are shot, the two images are displayed side by side immediately after shooting. When [Anti Blink] is displayed, 2 images are taken automatically and the image with the eyes open is selected automatically. [Details]

Notes

- Scene Recognition function does not operate when you use zoom functions other than the optical zoom.

- The available flash settings are [Auto] and [Off].

- These scenes may not be recognized depending on the situation.

- In Tracking focus mode, (Portrait), (Infant), (Night Portrait) or (Backlight Portrait) are not recognized.

- If the environment causes vibrations to be transferred to the camera when (Tripod) and (Night Scene) condition are recognized at the same time, (Tripod) conditions may not be recognized.

- Sometimes a slow shutter results when (Tripod) and (Night Scene) condition are recognized at the same time. Keep the camera still during shooting.

- When shooting movies, Advanced mode is not available.

### Advanced mode

In [Advanced] mode, the camera shoots two images consecutively with the different settings as follows when it recognizes (Night Scene), (Night Portrait), (Backlight) or (Backlight Portrait) scenes, which tend to blur or when (Night Scene) and (Tripod) conditions are recognized at the same time. You can select the desired image from the two images shot.

| First Image* | Second Image
| Shoots in Slow Synchro | Shoots with sensitivity increased and shake reduced
| Shoots in Slow Synchro with the face which the flash strobes on as guide | Shoots with sensitivity increased with the face as guide and shake reduced
| Shoots in Slow Synchro | Shoots with a slower shutter speed without increasing sensitivity
| Shoots with the flash | Shoots with the brightness and contrast of the background adjusted
| Shoots with the face which the flash strobes on as guide | Shoots with the brightness and contrast of the face and the background adjusted

* When [Flash] is set to [Auto].
What is the Anti Blink function?
When set to [Advanced], the camera automatically shoots two images consecutively* when it recognizes (Portrait) or (Infant). The camera will select, display, and record the image which the eyes are not blinked automatically. If the eyes are closed in both images, the message “Blinked eye detected” is displayed.
* except when the flash strobes/when the shutter speed is slow.
Related Topic
MENU items not available in some REC modes
Back to top