Cyber-shot User Guide
Print
Top page > Before Use > Names of parts and list of icons displayed on the screen > List of icons displayed on the screen

## List of icons displayed on the screen

List of shooting mode icons
List of viewing mode icons
Icons are displayed on the screen to indicate the camera status.
The displayed icon positions may differ according to the shooting mode.

### List of shooting mode icons

Display | Indication
0:12 | Recording time (m:s)
REC Standby | Recording a movie/Movie standby
| Movie shooting scene
| Scene Recognition icon (Close Focus) is displayed only for DSC-TX66.
| Database file full/Database file error
| Scene Recognition
| Overlay icon
| Anti Blink
| Overheating warning
| Vibration warning
| Drop sensor (DSC-WX70 only)
| White Balance
| Burst Shooting Interval
| Metering Mode
| Face Detection
| Defocus Effect
| Soft Skin Effect
| HDR Painting effect
| Color hue
| Extracted Color
| Watercolor effect
| Illustration effect

Display | Indication
| Close Focus (DSC-TX66 only)
| Red-eye reduction
| AE/AF lock
| NR slow shutter
125 | Shutter speed
F3.5 | Aperture value
ISO400 | ISO number
+2.0EV | Exposure value
| AF range finder frame indicator
| Flash mode
| Flash charging

Display | Indication
| Eco mode
9 | Number of recordable images (Dual Rec)
| Battery remaining
| Low battery warning
1.4 | Zoom scaling
CAPTURE | Importing still images
| AF Illuminator
| Recording Media (Memory card, internal memory)

Display | Indication
100Min | Recordable time
C:32:00 | Self-diagnosis display
| Recording folder
| Image size/Panorama image size/Quality (16M) and (16:9(12M)) are displayed only for DSC-WX70. (18M) and (16:9(13M)) are displayed only for DSC-TX66.
| AF range finder frame
| Spot metering cross-hairs
| Self-timer
| Warning indicator pertaining to still image recording
96 | Number of recordable images
| Write Date
| Destination
| Touch panel invalid
| Enable/Disable touch panel
| Histogram (DSC-WX70 only)

### List of viewing mode icons

Display | Indication
| Playback Media (Memory card, internal memory)
12/12 | Image number/Number of images recorded in selected date range, folder
| Image size/Panorama image size/Quality (16M) and (16:9(12M)) are displayed only for DSC-WX70. (18M) and (16:9(13M)) are displayed only for DSC-TX66.
| Burst Images
| Main image in the burst group
| Playback zoom
| Playback folder
| Database file full/Database file error
| 3D images
| Protect
| Print order (DPOF)
| Overheating warning
| TransferJet settings (DSC-WX70 only)
| Enlargement unavailable
| Eye-Fi (DSC-WX70 only)

Display | Indication
101-0012 | Folder-file number
2012-1-1 9:30 AM | Recorded date/time of the playback image

Display | Indication
| Eco mode
| Battery remaining
| Low battery warning
| View mode
| Metering Mode
| Flash mode
| White Balance
+2.0EV | Exposure value
| Wide zoom

Display | Indication
C:32:00 | Self-diagnosis display
ISO400 | ISO number
500 | Shutter speed
F3.5 | Aperture value
| Playback bar
| Playback
| Variable speed playback
00:00:12 | Counter
| Histogram (DSC-WX70 only)
| Volume

Back to top