Cyber-shot User Guide
Print
Top page > Shooting > Setting REC mode > iSweep Panorama

## iSweep Panorama

Allows you to create a panoramic image from composite images. The camera also automatically detects people’s faces or moving subjects.

1. Set the camera to shooting mode.

1. (REC Mode) (iSweep Panorama)

1. Align the camera with the end of the subject to be shot and press the shutter button.

A: This part will not be recorded.
Touch B to change the shooting direction.

1. Pan the camera to the end of the guide (C), following the arrow indication on the screen.

Tips for shooting a panoramic image
Pan the camera in an arc at a constant velocity in the direction indicated on the screen. Subjects at rest are more suited for panorama shots than moving subjects.
Radius as short as possible.
Vertical direction
Horizontal direction

- First, press the shutter button halfway to lock the focus and exposure. Then, press the shutter button fully down and pan or tilt the camera.

- If a section with greatly varied shapes or scenery is concentrated along a screen edge, the image composition may fail. In such case, adjust the frame composition so that the section is in the center of the image, then shoot again.

Notes

- If you cannot pan the camera across the entire subject within the given time, a gray area occurs in the composite image. If this happens, move the camera faster to record a full panoramic image.

- Since several images are stitched together, the stitched part will not be recorded smoothly.

- When the whole angle of panoramic shooting and the AE/AF locked angle are very different in brightness, color and focus, the shooting will not be successful. If this happens, change AE/AF locked angle and shoot again.

- You cannot create panoramic images in the following situations:

- You pan the camera too quickly or too slowly.

- There is too much camera shake.

Related Topic
Scrolling the panoramic images for display
Still Image Size/Panorama Image Size
Functions not available in some REC modes
MENU items not available in some REC modes
Back to top