# Utilizzo

# IC Recorder ICD-PX333/PX333F

## Impostazioni Scene Select

Le voci di impostazione per il menu Scene Select sono impostate sui valori seguenti.

#### Meeting

REC Mode: 192kbps (MONO) (SHQ)

Mic Sensitivity: Medium

VOR: OFF

LCF(Low Cut): ON

Select Input: MIC IN

#### Voice Notes

REC Mode: 128kbps (MONO) (HQ)

Mic Sensitivity: Low

VOR: OFF

LCF(Low Cut): ON

Select Input: MIC IN

#### Interview

REC Mode: 192kbps (MONO) (SHQ)

Mic Sensitivity: Medium

VOR: OFF

LCF(Low Cut): ON

Select Input: MIC IN

#### Lecture

REC Mode: 192kbps (MONO) (SHQ)

Mic Sensitivity: Medium

VOR: OFF

LCF(Low Cut): OFF

Select Input: MIC IN

#### Audio IN

REC Mode: 192kbps (MONO) (SHQ)

Mic Sensitivity: Low

VOR: OFF

LCF(Low Cut): ON

Select Input: Audio IN

#### Nota

- Non è possibile modificare le impostazioni Scene Select. Se si desidera modificare le voci delle impostazioni, ad esempio Modalità reg., Sensibilità mic. e così via in base alle situazioni di registrazione, utilizzare il menu per modificare ciascuna di esse.

### Argomento correlato

- Selezione di una scena di registrazione per ogni situazione