# How to Use

# IC Recorder ICD-PX333/PX333F

## Erasing a track mark

You can erase the track mark that is located at just before the current position.

1. Stop at a position after the track mark you would like to erase.
2. In the stop mode, select DISP/MENU - “Delete” - “Erase Track Mark,” and then press PLAY/STOP・ENTER.

   “Erase Track Mark?” is displayed and the track mark indicator and the track mark number to be erased will flash.

3. Press – or + to select “YES,” and then press PLAY/STOP・ENTER.

   The “Erasing...” animation appears in the display window and the selected track mark will be erased.

   A. Before erasing a track mark: is the stop position.

   B. After erasing a track mark: The track mark just before the stop position will be erased.

4. Press (stop) to exit the menu mode.

#### Note

- You cannot erase track marks from a protected file. To erase track marks from the file, release the protection first, and then erase the track marks.

#### Hint

- To cancel erasing, select “NO” in step 3, and then press PLAY/STOP・ENTER.

### Related Topic

- Protecting a file