# How to Use

# IC Recorder ICD-PX333/PX333F

## Inserting a memory card

In addition to the built-in memory,you can record files on a memory card.

#### Note

- In this Help Guide, M2™ and microSD cards are generally referred to as a “memory card.” The M2™/microSD card slot is referred to as the “memory card slot.”

1. Open the cover of the memory card slot in the stop mode.

2. Insert an M2™ card with the terminal side facing toward you () (*), or insert microSD card with the label side facing toward you () (*), securely to the end of the slot until it clicks into place.

   * When you are inserting a memory card with the back side of the IC recorder facing toward you.

3. Close the cover.

#### Note

- Do not insert or remove a memory card during recording/playback/formatting.

  Doing so may cause a malfunction of the IC recorder.

- Do not remove a memory card while the “Accessing...” animation appears in the display window. Doing so may damage the data.
- If a memory card is not recognized, remove it and then insert it into the IC recorder again.
- Close the cover of the memory card slot firmly. Also, do not insert any liquid, metal, flammable or any object other than a memory card into the slot. Doing so may cause fire, electric shock, or malfunctions.
- Before recording, we recommend that you copy all the data stored on the memory card to your computer and format the memory card on the IC recorder so it contains no data.

#### Hint

- To remove the memory card, push the memory card into the slot. When it pops out, remove it from the memory card slot.

### Related Topic

- Selecting the memory
- Formatting the memory (Format)
- Structure of folders and files
- About compatible memory card