# How to Use

# IC Recorder ICD-PX333/PX333F

## Display when recording

#### Note

- The window shown above displays indications, numbers or items for explanatory purposes. The actual window may differ from those displayed here.

1. Recording progress animation display

   Displays the progress of a recording in animation.

2. Recording indicator

   Appears while the IC recorder is recording

3. VOR recording indicator

   Appears when “VOR” is set to “ON” in the menu.

4. Scene select indicator

   Displays the currently selected scene used for recording. Appears when a scene is set.

   : Meeting

   : Voice Notes

   : Interview

   : Lecture

   : Audio IN

5. LCF (Low Cut Filter) indicator

   Appears when “LCF(Low Cut)” is set to “ON” in the menu.

6. Microphone sensitivity indicator

   Displays the microphone sensitivity that has been set in the menu.

   : High

   : Medium

   : Low

7. Recording mode indicator

   Recording mode indicator Displays the recording mode set in the menu when the IC recorder is in the stop or recording mode, and displays the current recording mode when the IC recorder is in the playback mode:

   SHQ: Super high-quality monaural recording mode (192kbps(MONO))

   HQ: High-quality monaural recording mode (128kbps(MONO))

   SP: Standard play monaural recording mode (48kbps(MONO))

   LP: Long play monaural recording mode (8kbps(MONO))