# How to Use

# IC Recorder ICD-PX333/PX333F

## Preventing unintentional operations (HOLD)

You can disable all the buttons (HOLD) in order to prevent unintentional operations when you carry the IC recorder, etc.

1. Slide the HOLD・POWER ON/OFF switch in the direction of “HOLD” to disable the buttons while the power is on.

   “HOLD” appears for approximately 3 seconds, indicating that all the button operations are disabled.

#### Note

- When the HOLD function is activated during recording, all button operations are disabled. To stop recording, cancel the HOLD function first.

#### Hint

- Even if the HOLD function is activated, you can stop the alarm playback by pressing any button. (You cannot stop normal playback.)

### Related Topic

- Releasing the HOLD function