# How to Use

# IC Recorder ICD-PX333/PX333F

## Selecting the recording mode (REC Mode)

You can set the recording mode for the files to be recorded. Set this menu item before you start recording.

1. In the stop mode, select DISP/MENU - “Detail Menu” - “REC Mode,” and then press PLAY/STOP・ENTER.

2. Press – or + to select the desired recording mode, and then press PLAY/STOP・ENTER.
3. Press (stop) to exit the menu mode.

#### Descriptions of menu items

You can select one of the menu items available.

192kbps(MONO):

Super high-quality monaural recording mode (displayed as “SHQ” in the window)

(Initial setting)

128kbps(MONO):

High-quality monaural recording mode (displayed as “HQ” in the window)

48kbps(MONO):

Standard play monaural recording mode (displayed as “SP” in the window)

8kbps(MONO):

Long play monaural recording mode (displayed as “LP” in the window)