# How to Use

# IC Recorder ICD-PX333/PX333F

## Scene Select settings

The setting items for the Scene Select menu are set as follows.

#### Meeting

REC Mode: 192kbps (MONO) (SHQ)

Mic Sensitivity: Medium

VOR: OFF

LCF(Low Cut): ON

Select Input: MIC IN

#### Voice Notes

REC Mode: 128kbps (MONO) (HQ)

Mic Sensitivity: Low

VOR: OFF

LCF(Low Cut): ON

Select Input: MIC IN

#### Interview

REC Mode: 192kbps (MONO) (SHQ)

Mic Sensitivity: Medium

VOR: OFF

LCF(Low Cut): ON

Select Input: MIC IN

#### Lecture

REC Mode: 192kbps (MONO) (SHQ)

Mic Sensitivity: Medium

VOR: OFF

LCF(Low Cut): OFF

Select Input: MIC IN

#### Audio IN

REC Mode: 192kbps (MONO) (SHQ)

Mic Sensitivity: Low

VOR: OFF

LCF(Low Cut): ON

Select Input: Audio IN

#### Note

- You cannot modify the Scene Select settings. If you want to change the setting items, such as REC Mode, Mic Sensitivity, etc., for recording situations, use the menu to change each item of recording settings.

### Related Topic

- Selecting a recording scene for each situation