# Kullanım Talimatları

# IC Recorder ICD-PX333/PX333F

## Scene Select ayarları

Scene Select menüsü için ayar öğeleri şu şekilde ayarlanır.

#### Meeting

REC Mode: 192kbps (MONO) (SHQ)

Mic Sensitivity: Medium

VOR: OFF

LCF(Low Cut): ON

Select Input: MIC IN

#### Voice Notes

REC Mode: 128kbps (MONO) (HQ)

Mic Sensitivity: Low

VOR: OFF

LCF(Low Cut): ON

Select Input: MIC IN

#### Interview

REC Mode: 192kbps (MONO) (SHQ)

Mic Sensitivity: Medium

VOR: OFF

LCF(Low Cut): ON

Select Input: MIC IN

#### Lecture

REC Mode: 192kbps (MONO) (SHQ)

Mic Sensitivity: Medium

VOR: OFF

LCF(Low Cut): OFF

Select Input: MIC IN

#### Audio IN

REC Mode: 192kbps (MONO) (SHQ)

Mic Sensitivity: Low

VOR: OFF

LCF(Low Cut): ON

Select Input: Audio IN

#### Not

- Scene Select ayarlarını değiştiremezsiniz. Kayıt şartlarına uygun olacak şekilde, REC Modu, Mikrofon Duyarlılığı vb. gibi ayar öğelerini değiştirmek istiyorsanız, her bir kayıt ayarını değiştirmek için menüyü kullanın.

### İlgili Konu

- Her durum için kayıt ortamı seçme