================ All PCI/PCIe 8110SC/8168 10/100/1000 NETWORK ADAPTER =============

Q. What is 'Shutdown Wake-On-Lan' ? Why have this feature ? Who requires to use this feature ?

A. This feature is for power consumption. This affects shutdown mode (S5) power consumption.

   When users change the setting to 'Disabled' and goes to shutdown,
   the driver will disable the PHY.

   PS. If this feature setting is disabled, wake-on-lan from shutdown will not work.
       If you want wake-on-lan from shutdown, please change the setting to enabled.


