VAIO User Guide

Task

# Replacing the AA Battery of the Remote Commander
<TV tuner board installed models>

If the remote commander does not operate properly, replace the batteries.

1. Turn over the remote commander and remove the battery compartment cover.

1. Remove both old batteries and insert two new AA batteries (minus (-) end of each battery first), then close the cover.

Note

- If the remote commander is not going to be used for an extended period of time, remove the batteries.

- Since the remote cannot be used with the commercially available rechargeable batteries, use the non-rechargeable AA batteries. If you use the rechargeable batteries, battery leakage may occur, resulting in a malfunction.

- When the battery power becomes low, replace with the battery promptly. Keeping depleted batteries in the remote may cause battery leakage.

- Do not recharge the dry cell AA batteries.